HENRY COUNTY ENGINEER

APPLICATON TO TILE OPEN DITCH

Please fill in any blanks, sign and send back to the County Engineer’s Office, via:

Email: [tschumm@henrycountyengineer.com](mailto:tschumm@henrycountyengineer.com) Fax: (419)592-5508

Address: 1823 Oakwood Avenue, Napoleon, Ohio 43545

Date: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Township: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Section: \_\_\_\_\_\_\_

Road: \_\_\_ between ROADS \_\_ and \_\_\_  North  East

APPROXIMATELY \_\_\_\_\_\_\_\_ ft.  South  West from \_

WHICH SIDE OF ROAD: \_\_\_\_\_\_\_ NO. OF ACRES \_\_\_\_\_

Draining through closed portion

PROPOSED TILE/PIPE LENGTH: \_\_\_\_\_\_ Linear Feet

REASONS FOR CLOSING:

Access to property

Applicant Signature: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_

Name Printed: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_

Address:  \_\_ \_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_

\_\_ \_

Email: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Telephone Number: \_\_\_\_\_\_\_\_\_\_\_\_\_\_

- - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - - -

SIZE OF PIPE REQUIRED: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

TYPE OF PIPE RECOMMENDED: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

REMARKS:



See 2nd page of application \_\_\_\_ APPROVED BY:

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

HENRY COUNTY ENGINEER

\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

By: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_ Deputy

Date:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

**COMMENTS FOR**

**APPLICATION TO TILE OPEN DITCH**

SIZE OF PIPE REQUIRED: \_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

TYPE OF PIPE RECOMMENDED:\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_\_

Pipe in open ditch shall be laid on (6”) inches of stone bedding. The material shall be No. 67 or No. 411 limestone conforming to the State of Ohio, Department of

Transportation Construction and Material Specification.

Finish grade of pipe invert (inside bottom) shall be approximately **\_\_\_\_\_\_\_**

below existing ditch grade.

Provide surface drainage away from road. Minimum slope shall be one (1”) inch per foot on seeded turf shoulders to centerline of existing ditch. Then grade ground from centerline of existing ditch to private property according to property owner’s requirement.

Acceptance of the final installation subject to the approval of the Henry County Department of Highways.

Notes: